INTERIOR SPOTS

What you are describing is what is known as Dirt Scale.

Basically, a thin layer of calcium build up has trapped the dirt on the

surface of the pool. This is the reason you cannot brush it away. It’s sort

of like painting a coat of polyurethane over a spot of dirt on the wall.

Unless you break down that calcium build up, that dirt is not going to

go away.

Most people only pay attention to how clear the water looks. If the

water is clear, the water chemistry is good. It’s not as simple as that,

but it is easy.

If you don’t already have one, get to your pool supply store and

purchase a chemical test kit. The test strips will work, but if you want a

more accurate test result, get a kit that includes the drops.

Once you have a test kit, you will want to test the water at least 2-3

times a week. The most important things to pay attention to are PH,

Total Alkalinity and Hardness. It is important to keep the PH around 7.2-

7.6 to avoid the build up your seeing.

BTW, THERE IS A VERY SIMPLY WAY TO GET RID OF THAT SCALE. IT

WILL TAKE SOME TIME BUT IT WILL WORK IF YOU PUT THE TIME AND

EFFORT INTO IT. ALL YOU NEED TO DO IS DROP YOUR PH LEVEL TO

ABOUT 6.8-7.0 AND BRUSH BRUSH BRUSH. TEST THE WATER EVEN MORE

FREQUENTLY DURING THE PROCESS. YOU PROBABLY WON’T NOTICE ANY

IMPROVEMENT RIGHT AWAY, BUT OVER THE COURSE OF A FEW WEEKS,

IT WILL START TO FADE AWAY.